This update package is used to update E65 and E80 grinders with WIFI FW <116 to the newest WIFI and Grinder firmware.
After this update the grinder is compatible with the normal update images.
ATTENTION: This update package is not for grinders that have already been updated.
Should you for any reason install the wifiupdater binary on any machine that doesn't need it, it can be recovered using the WifiUpdater.exe, selecting "y" at step 2. If it fails the display board needs to be returned to the factory for reflashing.

Step 1: Enable WIFI on the grinder and connect to the WIFI E65... , E80... or Wave2_Fallback... using the password "e65sgbwdemo" 

Step 2:	Run the included WifiUpdater.exe file and type "n" without " and press enter.

Step 2b: If you already have run the WifiUpdater and it failed, check if the one of the WIFIs mentioned in step 1 are still available.
		 If they are continue with "n". 
		 If you are seeing the "NG_WIFIUPDATER" wifi, connect to it using the password "e65sgbwdemo" and choose "y". Continue at step 4.
		 Should you not be able to connect to any of these WIFI networks, the display board needs to be returned to the factory for reflashing.
		 
Step 3: Wait for the WIFI updater to signal a sucessful upload and continue with displayed instructions.
		If it says "file upload failed" you can try again from Step 1.		

Step 4: The Updater will upload and install the newest included WIFI image. Do not turn off the grinder or the WIFI Please wait for at least 5 minutes to see the WIFI available.
		DO NOT REMOVE POWER FROM THE GRINDER!
		Should this fail and neither of the WIFIs followed
		E65... , E80... or Wave2_Fallback...
		or
		NG_WIFIUPDATER
		are available, the display board needs to be returned to Mahlkönig Service for reflashing.
		
Step 5: If successful you should be able to connect to the E65... , E80... or Wave2_Fallback... WIFIs and install the newest 
		included grinder firmware in the webinterface entering 192.168.4.1 in your browser.
		

